**Teflon PTFE** (polytetrafluoroethylene) A nonstick coating with one of the highest operating temperature of any fluoropolymer products. (260 C/500 F. Has an extremely low coefficient of friction, good abrasion resistance, and good chemical resistance.